AED71-8N, Input file: http://farbe.li.tu-berlin.de/AED7/AED70-1N.EPS, 1MR, gamma gP=2,105, CYP15=CYN1

AED70-3, picture A1Wdd: Element A: radial gratings N-W, W-N, N-Z, and W-Z; PS operator: rgb/cmy0/w/000n radial gratings (Siemens-stars) N-Z

10 20 30

radial gratings (Siemens-stars) N-W

10 20 30

radial gratings (Siemens-stars) W-N

10 20 30

radial gratings (Siemens-stars) W-Z

10 20 30

AED70-5, picture A2Wdd: Element B: 5 visual equidistant L*-grey steps + N0 + W1; PS operator: rgb/cmy0/w/000n

L*/Y_{input}

(absolute)

w*=l*_{CIELAB, r}

(relative)

w*_{input}

AED70-7, picture A3Wdd: Element C: 16 visual equidistant L*-grey steps; PS operator: rgb/cmy0/w/000n

L*/Y_{input}

(absolute)

No. and Hex code

w*=l*_{CIELAB, r}

(relative)

w*_{input}

AED71-1, picture A4Wdd: Element D: Landolt-rings W-N; PS operator: rgb/cmy0/w/000n background step Hex code

Landolt-rings W-N ring step Hex code

code: background - ring

AED71-3, picture A5Wdd: Element E: Line raster under 45o (or 135o); PS-operator: rgb/cmy0/w/000n line raster diameter in lpi

AED71-5, picture A6Wdd: Element F: Line raster under 90o (or 0o); PS-operator: rgb/cmy0/w/000n line raster diameter in lpi