Fe39-1, olv*

Fe391-1, Picture B4: 16 equidistant steps W-C, W-M, W-Y, W-N; PS operator olv* setrgbcolor

Fe390-3, Picture B1: Flower motif, 14 CIE-test colours, 16 grey steps (sf); PS operators settransfer, 4 colorimage

image pixel: 192 x 128 384 x 256 768 x 512 1536 x 1024 3072 x 2048

Fe391-3, Picture B5: Script and Landolt-rings N, C, M, Y, Z; PS operator olv* setrgbcolor

Fe391-5, Picture B2: Radial gratings PS operator olv* setrgbcolor Fe391-5, Picture B6: Landolt-rings W-C, W-M; PS operator olv* setrgbcolor

Fe390-7, Picture B3: 14 CIE-test colours and 2 + 16 grey steps; Use of PS operator olv* setrgbcolor Fe391-7, Picture B7: Landolt-rings W-Y, W-N; PS operator olv* setrgbcolor

-8 -6 -8 -6

-8 -6 -8 -6

Fe39-1; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705 Fig. B1 to B7 similar ISO/IEC-Test chart 2, olv* interpretation input: rgb->olv* setrgbcolor output: no change compared to input www.ps.bam.de/Fe39/10Y/Y10100NP.PS./PDF, Page 1/6; ORS20_95, L*=20_95; start output N: No Output Linearization (OL) data in File (F), Startup (S) or Device (D)

See for similar files: http://www.ps.bam.de/Fe39/; www.ps.bam.de/Fe.HTM Technical information: http://www.ps.bam.de

Version 2.1, io=1,1, ColSpx=1 BAM registration: 20081001-Fe39/10Y/Y10100NP.PS./PDF BAM material: code=rha4ta application for evaluation and measurement of printer or monitor systems

Fe39-2, olv*

Fe390-1, Picture B4N: 16 equidistant steps N-C, N-M, N-Y, W-N; PS operator olv* setrgbcolor

Fe391-1, Picture B4Z: 16 equidistant steps Z-C, Z-M, Z-Y, W-N; PS operator olv* setrgbcolor

Fe390-3, Picture B5N: Script and Landolt-rings W, C, M, Y, Z; PS operator olv* setrgbcolor Fe391-3, Picture B5Z: Script and Landolt-rings N, C, M, Y, W; PS operator olv* setrgbcolor

Fe390-5, Picture B6N: Landolt-rings N-C, N-M; PS operator olv* setrgbcolor Fe391-5, Picture B6Z: Landolt-rings Z-C, Z-M; PS operator olv* setrgbcolor

Fe390-7, Picture B7N: Landolt-rings N-Y, W-N; PS operator olv* setrgbcolor Fe391-7, Picture B7Z: Landolt-rings Z-Y, W-N; PS operator olv* setrgbcolor

-8 -6 -8 -6

-8 -6 -8 -6

Fe39-2; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705 Fig. B4 to B7 similar ISO/IEC-Test chart 2, olv* interpretation input: rgb->olv* setrgbcolor output: no change compared to input www.ps.bam.de/Fe39/10Y/Y10100NP.PS./PDF, Page 1/6; ORS20_95, L*=20_95; start output N: No Output Linearization (OL) data in File (F), Startup (S) or Device (D)

See for similar files: http://www.ps.bam.de/Fe39/; www.ps.bam.de/Fe.HTM Technical information: http://www.ps.bam.de Version 2.1, io=1,1, ColSpx=1 BAM registration: 20081001-Fe39/10Y/Y10100NP.PS./PDF BAM material: code=rha4ta application for evaluation and measurement of printer or monitor systems

Fe39-3, olv*

Fe391-1, Picture D4: 16 equidistant steps W-O, W-L, W-V, W-N; PS operator olv* setrgbcolor

Fe390-3, Picture B1: Flower motif, 14 CIE-test colours, 16 grey steps (nf); PS operators settransfer, 4 colorimage Fe391-3, Picture D5: Script and Landolt-rings N, O, L, V, Z; PS operator olv* setrgbcolor

Fe391-5, Picture D2: Radial gratings PS operator olv* setrgbcolor Fe391-5, Picture D6: Landolt-rings W-O, W-L; PS operator olv* setrgbcolor

Fe390-7, Picture D3: 14 CIE-test colours and 2 + 16 grey steps; Use of PS operator olv* setrgbcolor Fe391-7, Picture D7: Landolt-rings W-V, W-N; PS operator olv* setrgbcolor

Fe39-3; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705 Fig. D1 to D7 similar ISO/IEC-Test chart 4, olv* interpretation

Fe39-4, olv*

Fe390-1, Picture D4N: 16 equidistant steps N-O, N-L, N-V, W-N; PS operator olv* setrgbcolor

Fe391-1, Picture D4Z: 16 equidistant steps Z-O, Z-L, Z-V, W-N; PS operator olv* setrgbcolor

Fe390-3, Picture D5N: Script and Landolt-rings W, O, L, V, Z; PS operator olv* setrgbcolor Fe391-3, Picture D5Z: Script and Landolt-rings N, O, L, V, W; PS operator olv* setrgbcolor

Fe390-5, Picture D6N: Landolt-rings N-O, N-L; PS operator olv* setrgbcolor Fe391-5, Picture D6Z: Landolt-rings Z-O, Z-L; PS operator olv* setrgbcolor

Fe390-7, Picture D7N: Landolt-rings N-V, W-N; PS operator olv* setrgbcolor Fe391-7, Picture D7Z: Landolt-rings Z-V, W-N; PS operator olv* setrgbcolor

Fe39-4; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705 Fig. D4 to D7 similar ISO/IEC-Test chart 4, olv* interpretation

Fe39-6, olv*

Fe390-3, Picture B1: Flower motif, 14 CIE-test colours, 16 grey steps (sf6); PS operators settransfer, 4 colorimage

Fe39-6; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705

Fe39-7, olv*

Fe39-7; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705

Fe39-8, olv*

Fe390-3, Picture B1: Flower motif, 14 CIE-test colours, 16 grey steps (nf6); PS operators settransfer, 4 colorimage

Fe39-8; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705

Fe39-9, olv*

Fe39-9; Test elements of ISO/IEC 15775 and ISO/IEC TR 24705

Fe39-5, olv* ColSpx=1 colorm=0 xcharti=0 xcharts=4 DEintp=0, (A-a, k-n), DEintp=1, (b-j)