JE030-7N, Colorimetric data of Television Luminous System TLS for CIE lightness L*= for CIE standard illuminant D65; LECD monitor; Page: 1/20

Colorimetric "Standard data": Television Luminous System TLS for CIE lightness L*= of black for illuminant D65 System TLS; LECD monitor (with LED backlight)

rgb=olv* cmy0* no. position L*=LAB*1 a*=LAB*2 b*=LAB*3 C*ab=LAB*r hab X=XYZ1 Y=XYZ2 Z=XYZ3 x y Y/88.59