KE890-7A KE890-7A, 2

Interpretation rgb -> rgb* and CIELAB data of a 48 step elementary hue circle for a sRGB standard display with the luminance reflection L_r=10% compared to the white reference (100%) 48 step elementary hue circle with hues: RJGB: h_{ab,a} = 25.5, 92.3, 162.2, 271.7, and C’ M’ = 217, 328.6 Comparison with six device hues OYLCVM: h_{ab,a} = 9 step equidistant grey scale: L* =