OE990-7N, Page 1/16, Test chart 2E with 40x27=1080 colours; digital equidistant 9 or 16 step colour scales; Colour data in column (A-n): rgb + cmy0 (A_j + k26_n27), 000n (k), w (l), nnn0 (m), www (n), colorm = 0, xchart = 0, pchart = 0

OE940-7A, Picture B1-030-0: Flower motif, 14 CIE-test colours and 2+16 grey steps (sf); PS operators settransfer, 3 colorimage

image pixel: 192 x 128 384 x 256 768 x 512 1536 x 1024 3072 x 2048

Part 3 OE990-7A-030-1

Documentation of file format, hardware and software for this test:

PDF-File: http://130.149.60.45/farbmetrik/OE99/OE99L0NP.PDF underline Yes/No

PS-File: http://130.149.60.45/farbmetrik/OE99/OE99L0NA.PS or underline Yes/No

Used computer operating system: either one of Windows/Mac/Unix/other and version:................................. This evaluation is for the device output: underline monitor/data projector/printer Device model, driver and version:...................... Device output with PDF/PS-file: underline PDF/PS-file For device output with PDF-file OE99L0NP.PDF:

either PDF-file transfer "download, copy" to PDF device................................. or with computer system interpretation by "Display-PDF":................................. or with software. e. g. Adobe-Reader/-Acrobat and version:................................. or with software e. g. Ghostscript and version:.................................

For device output with PS-file OE99L0NA.PS:

either PS-file transfer "download, copy" to PS device................................. or with computer system interpretation by "Display-PS":................................. or with software e. g. Ghostscript and version:................................. or with software e. g. Mac-Yap and version:.................................

Special remarks:Special remarks, e. g. output of Landscape (L) ...................................................................... ...................................................................... ......................................................................

OE990-7A, Picture A7-030-2: 16 visual equidistant L*-grey steps; PS operator: w* w* w* setrgbcolor

L*/Y_{intended}

(absolute)

w*=l*_{CIELAB, r}

(relative)

No. and Hex code w* w* w* setrgb gP=1.00

w*_{intended} w*_{out}