SE880-7N Measurement: %BEG ’KK0X’REM_OFFS04_080929_3.TXTOffset print, model separation cmyn6*, Page 1/2

48 step circle with interpretation rgb -> rgb*_d device hue steps of 1080 standard colours

RYGB_{ton}, 25.4, 92.3, 162.2, 271.7 RYGB_{all}: LAB*Nio: , , LAB*Wio: , ,

16 step elementary hue circle with intended elementary hues: h_{ab,a} = 25.4, 92.3, 162.2, 271.7 X Y Z x y h_{AB} L* a* b* L*_a a*_a b*_a C*_{ab,a} h_{ab,a} rgb -> rgb*_e

5 step equidistant grey scale with intended lightness: L* = , , , ,