AEN70-7N,

TLS18 Reflection colorimetry, System WCGa, L*ABJND-L*ABCh, Y_{Nn} = 2.52, L*_{Nn} = 18.01, Y_{Za} = 18,0 Colour