EE680-3N

Input Output Input and output media and applications

Input media Output media Application

Technical Report (TR) or Standard

Method & Test: Linearization

- - - - Basis ISO/IEC TR 24705 DIN 33866-1DIN 33872-1

analog^{2)} analog

ISO/IEC-file series equally spaced in rgb* ISO/IEC-test chart (hardcopy) series equally spaced in LCh*

Hardcopy Copier ISO/IEC 15775^{2)} DIN 33866-2^{2)} JIS X 6933^{1) 2)}

analog^{2)} digital ISO/IEC-test chart (hardcopy) series equally spaced in Lch* File Scanner ISO/IEC TR 24705 DIN 33866-4

digital^{1)} analog ISO/IEC-test chart (File) series equally spaced in rgb*

Hardcopy Printer ISO/IEC TR 24705

DIN 33866-3 DIN 33872-2,4

Softcopy Display ISO/IEC TR 24705 ISO 9241-306:2018^{1)}

DIN 33866-5 DIN 33872-2,4

1) Digital ISO-test files for free download from: http://standards.iso.org/iso/9241/306/ed-2/index.html 2) Analog ISO-test charts are available from 3 sources: DIN 33866-2, JIS X 6933, Richter, 2012, offset print (3600dpi), siehe Colour and Colour Vision, compare as file http://standards.iso.org/iso/9241/306/ed-2/ES15.PDF

ISO/IEC-input linearization method ISO/IEC-output linearization method, OUTLIN16_01.PDF

Input Output Application Technical Report (TR) or Standard

Input Output media

Application Technical Report (TR) or Standard

Original scene + CIE colours

ISO/IEC Image File

Reference Image File

ISO/IEC 15775^{2)}

ISO/IEC TR 24705

ISO/IEC File

Hardcopy Printer ISO/IEC TR 19797

ISO/IEC File

Softcopy Display ISO 9241-306:2018 8 viewing conditions

ISO/IEC File

Softcopy Display

Hardcopy Offset

Hardcopy Printer

CIE R8-09:2015 (CIE internal) + http:/ /farbe.li.tu-berlin.de /OUTLIN16_01.PDF