fea11-1n

Colour Management, based on ISO 9241-306:2018

rgbd=729 colour device data to device hue data rgb’ddi=visual equally spaced device output (i=1,2,3) all 3 displays: device output contrast range ISO CY5: 2,5≤Y≤90 ISO rgb* PCS PCC AE49